|  |
| --- |
| **I (38054) chip[DIS]: Advertise operational node 80159371E78DC854-8895951A5C0881BA**  **E (38054) chip[SVR]: Operational advertising failed: 3**  **I (38194) chip[DL]: Confirm received for CHIPoBLE TX characteristic indication (con 0) status= 14**  **I(39194) OPENTHREAD:[N] Ip6-----------: Bad UDP checksum**  **W(39194) OPENTHREAD:[W] Ip6-----------: Failed to handle payload: Drop**  **I (39264) chip[DL]: Write request/command received for CHIPoBLE TX CCCD characteristic (con 0 ) indicate = 0**  **I (39264) chip[DL]: CHIPoBLE unsubscribe received**  **I (39264) chip[DL]: BLE GAP connection terminated (con 0 reason 0x213)**  **I (39264) chip[BLE]: Releasing end point's BLE connection back to application.**  **I (39264) chip[DL]: Closing BLE GATT connection (con 0)**  **E (39274) chip[DL]: ble\_gap\_terminate() failed: Error CHIP:0x00000048**  **I (39274) esp\_matter\_core: BLE Disconnected**  **E (40554) chip[DL]: SRP update error: timed out waiting on server response**  **I(41194) OPENTHREAD:[N] Ip6-----------: Bad UDP checksum**  **W(41194) OPENTHREAD:[W] Ip6-----------: Failed to handle payload: Drop**  **W(41624) OPENTHREAD:[W] DuaManager----: Failed to perform next registration: NotFound** |