|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Test your product**  Try your created product on your device right now |  |  | **Device Status**  Check your connected device's info |
| Scan the below QR Code from any of the Matter supported phone apps (details below) to setup the device.  Note: Use the QR Code in the device's respective folder if you are flashing multiple devices yourself.  qr_code | |  | **Connected**  **ESP32-C6 (revision 0)**  ESP32-C6 (revision 0)   |  |  | | --- | --- | | **MAC** | 40:4C:CA:49:74:E0 | | **Features** | Wi-Fi 6, BT 5, IEEE802.15.4 | | |
|  |  | **Configuration Summary** Verify your device type and its configurations |
|  |  | **Device  Plug**  Indicator: WS2812 |
|  |  | **Module**  **ESP32-C6-DevKitM-1** |
|  |  | **driver**  **Input Button**  1000 / gpio / gpio\_config - Active high: No - IO pin GPIO: 9  **Output Relay**  1001 / gpio / gpio\_config  - Active high: No  - IO pin GPIO: 4  **LED**  1002 / ws2812 / ws2812\_config  - IO pin GPIO: 8 - Number of LEDs: 1 |